Introduction
============

The RK3399-Q7 (Puma) is a system-on-module featuring the Rockchip
RK3399 in a Qseven-compatible form-factor.

RK3399-Q7 features:
	* CPU: ARMv8 64bit Big-Little architecture,
		* Big: dual-core Cortex-A72
		* Little: quad-core Cortex-A53
		* IRAM: 200KB
	* DRAM: 4GB-128MB dual-channel
	* eMMC: onboard eMMC
	* SD/MMC
	* GbE (onboard Micrel KSZ9031) Gigabit ethernet PHY
	* USB:
		* USB3.0 dual role port
		* 2x USB3.0 host, 1x USB2.0 host via onboard USB3.0 hub
	* Display: HDMI/eDP/MIPI
	* Camera: 2x CSI (one on the edge connector, one on the Q7 specified CSI ZIF)
	* NOR Flash: onboard SPI NOR
	* Companion Controller: onboard additional Cortex-M0 microcontroller
		* RTC
		* fan controller
		* CAN

Here is the step-by-step to boot to U-Boot on rk3399.

Get the Source and build ATF binary
===================================

  > git clone https://git.trustedfirmware.org/TF-A/trusted-firmware-a.git

Compile the ATF
===============

  > cd trusted-firmware-a
  > make CROSS_COMPILE=aarch64-linux-gnu- PLAT=rk3399 bl31
  > cp build/rk3399/release/bl31/bl31.elf ../u-boot/bl31.elf

Compile the U-Boot
==================

  > cd ../u-boot
  > make CROSS_COMPILE=aarch64-linux-gnu- puma-rk3399_defconfig all

Flash the image
===============

Copy u-boot-rockchip.bin to offset 32k for SD/eMMC.
Copy u-boot-rockchip-spi.bin to offset 0 for NOR-flash.

SD-Card
-------

  > dd if=u-boot-rockchip.bin of=/dev/sdb seek=64

eMMC
----

rkdeveloptool allows to flash the on-board eMMC via the USB OTG interface with
help of the Rockchip loader binary.

  > git clone https://github.com/rockchip-linux/rkdeveloptool
  > cd rkdeveloptool
  > autoreconf -i && ./configure && make
  > git clone https://github.com/rockchip-linux/rkbin.git
  > cd rkbin
  > ./tools/boot_merger RKBOOT/RK3399MINIALL.ini
  > cd ..
  > ./rkdeveloptool db rkbin/rk3399_loader_v1.25.126.bin
  > ./rkdeveloptool wl 64 ../u-boot-rockchip.bin

NOR-Flash
---------

rkdeveloptool allows to flash the on-board SPI via the USB OTG interface with
help of the Rockchip loader binary.

  > git clone https://github.com/rockchip-linux/rkdeveloptool
  > cd rkdeveloptool
  > autoreconf -i && ./configure && make
  > git clone https://github.com/rockchip-linux/rkbin.git
  > cd rkbin
  > ./tools/boot_merger RKBOOT/RK3399MINIALL_SPINOR.ini
  > cd ..
  > ./rkdeveloptool db rkbin/rk3399_loader_spinor_v1.25.114.bin
  > ./rkdeveloptool ef
  > ./rkdeveloptool wl 0 ../u-boot-rockchip-spi.bin
